**2LINE Athene BOX**

Optical telecommunication outlet / Customer line termination

Optical termination point or customer connection box in single and multiple family homes

* For fixation on the wall or on flush-mounted boxes
* As a conversion point from outdoor to in-house cable and as a subscriber connection socket in the home
* Holds up to 3 couplings and 12 splices
* Capacity of 3x SC- Pigtails or 6x LC-Pigtails
* Tube/cable entry and fixation up to max. Ø10mm
* Use of gas/water - stop
* Fibre routing according to bending radii with the possibility of depositing excess fibre lengths
* Cable entry from below or from the rear with sealing and integrated strain relief
* Closing self-locking, by means of Torx screw or seal against unauthorized opening
* Hinged, latching cover
* Exchangeable splice holder for storing shrink or crimp splice protection elements
* Can be combined with cable excess length box for use with assembled cables

**Scope of delivery**

* Splice protection holder 12x crimp or 6x shrink
* Cable entry sleeve with membrane (max.Ø7mm)
* Cable ties
* Screws for fastening the aramid yarn
* Locking Torx screws
* Assembly instruction
* Wall fixation material (Universal plugs and screws)
* Adapters and pigtails included (yellow) (optional)
* Customer logo (optional)

**Varianten**

Item: 2LINE Athene KÜB

**Tests/Standards**

Protection Index IP20

Impact resistant IK07

Self-extinguishing according to UL94 V0 and UV-resistant

**Material**

Plastic, signal white RAL 9003

**Dimensions**

HxWxD[mm]: 135x96x27

**Article Code**

2LINE Athene BOX

**Article number**

21073

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99