**2LINE Network Distributor NVt 48**

Fibre optic network distributor

<div>Passive distribution point in FTTx fibre optic network&nbsp;</div><ul><li>Housing and base made of glass fibre reinforced 100% recyclable polycarbonate, coated in RAL 7038 with environmentally friendly paint&nbsp;</li><li>Central grounding point&nbsp;</li><li>Door with swivel lever, prepared for installation of a half profile cylinder&nbsp;</li><li>Base with detachable front flap and C-rail for fixing the tube assemblies&nbsp;</li></ul><div><br></div><ul><li>Interior fittings swivel frame with E&amp;MMS cassette system and fibre management&nbsp;</li><li>Inner rear panel for tube and cable management with cable excess length storage&nbsp;</li><li>Fixation of incoming cables with central element retention&nbsp;</li><li>Excess length storage of unused or uncut loose tubes (loop function)&nbsp;</li><li>Excess length storage of outgoing cables&nbsp;</li><li>Transfer and interception of cables in the splice area&nbsp;</li><li>Protected guiding of the loose tubes to the splicing area&nbsp;</li><li>Integration of splitters possible</li></ul>

**Scope of delivery**

* 1 pc. 2LINE NVt 48
* Splice cassette system 1-row with max. 72 locking places for up to 864 crimp splice or 864 shrink splice protection trays
* Sealed base plate with draught excluder for outlet area

**Varianten**

: NVt 24

**Tests/Standards**

Environmental protection class IP54

Security level breakage resistance (according to DIN 47609): T3

**Material**

Polycarbonate

**Dimensions**

Housing incl. base HxWxD[mm]: 1635x308x215

**Article Code**

2LINE NVt 24

**Article number**

22141

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99