**2LINE Network Distributor NVt 82**

Fibre optic network distributor

Passive distribution point in FTTx fibre optic network

* Housing and base made of glass fibre reinforced 100% recyclable polycarbonate, coated in RAL 7038 with environmentally friendly paint
* Central grounding point
* Door with swivel lever, prepared for installation of a half profile cylinder
* Base with detachable front flap and C-rail for fixing the tube assemblies
* Interior fittings swivel frame with E&MMS cassette system and fibre management
* Inner rear panel for tube and cable management with cable excess length storage
* Fixation of incoming cables with central element retention
* Excess length storage of unused or uncut loose tubes (loop function)
* Excess length storage of outgoing cables
* Transfer and interception of cables in the splice area
* Protected guiding of the loose tubes to the splicing area
* Integration of splitters possible

**Scope of delivery**

* Splice cassette system 2-row with max.144 locking places for up to 1.728 crimp splice or 864 shrink splice protection trays
* Sealed base plate with up to 8 feed-throughs for tube bundles and additional cable glands: outlet: 192x 7mm or 96x 10mm micro pipes; access: 3.5 - 20mm
* 1 pc. 2LINE NVt 82

**Tests/Standards**

Environmental protection class IP55

Impact resistance class IP54

**Material**

Glass fibre reinforced polycarbonate, aluminum, stainless steel

**Dimensions**

Housing HxWxD[mm]: 998x754x310; base HxWxD[mm]: 1060x754x284

**Article Code**

2LINE NVt 82

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99