**2LINE Iris+ BOX**

Subscriber connection box

Optical subscriber connection box for terminating the fibre in the home

* For mounting on the wall, on a DIN rail or as a flush-mounted box is possible
* Accommodates max. 2 couplings and 12 splice connections
* Holds 2x SC pigtails or 4x LC pigtails
* Cable entry max. Ø7mm from the rear or from below with sealing and integrated or optional additional strain relief
* Self-locking closure and safety adhesive strip to prevent unauthorised opening
* Hinged, latching cover
* Bending radius-compatible fibre guide with storage option for excess fibre lengths
* Replaceable splice holder for storing shrink or crimp splice protectors

**Scope of delivery**

* Couplings and pigtails (yellow) included (optional)
* 1 pc. 2LINE Iris⁺ BOX (with integrated splice protection holder)
* 1 pc. Cable entry grommet with membrane (max. Ø7mm)
* 4 pcs. screws for strain relief at aramid yarn
* 1 pc. cable tie
* 1 set of wall fixing (universal dowels and screws)
* 1 pc. transparent window and label (printing according to customer's requirements possible)
* 1 pc. safety adhesive strip
* 1 pc. screw and nut for lock
* Assembly instructions via QR code
* DIN - rail (optional)
* Strain relief element (optional)

**Tests/Standards**

Protection class IP40

Impact resistance IK07

Fire protection class UL94 V0

**Material**

Plastic PC / ABS, self-extinguishing according to UL94 V0, UV-resistant

**Dimensions**

HxWxD[mm]: 120x80x25

**Article Code**

2LINE Iris<sup>+</sup> BOX

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99