LC patch cable system

For plug connection between 2-LINE G-BOX and house connection

For the creation of a customer connection and for simple plug connection between 2-LINE G-BOX and customer building in the soil. Equipped with six optical fibers, two of which have LC/APC connectors. Adapted cable length, suitable for the 2LINE G-BOX KÜB, for protected storage of the excess length in the sealed housing. Longitudinally watertight along the entire cable length.

Scope of delivery
Tests/Standards

IP68



Article Code
2LINE G-BOX CAB LC

Brand: ZweiCom-Hauff GmbH
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