**corrugated pipe set**

For entry into the pylon marker

For protected installation of the 2-LINE G-BOX cable system or a fiber optic cable up to the pylons. Features: Length 0.75 m, clip on both sides for connection to the 2LINE G-BOX, sealing grommet on one side.

**Scope of delivery**

* 2 pieces of corrugated pipe connection coupling
* 1 piece of rubber bushing
* 0.75 m corrugated pipe ID 24 mm

**Article Code**

2LINE G-BOX WR SET

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99