**Membrane injection system**

for buildings without a basement

For reliable sealing of fibre optic cables. For installation in all standard wall types to DIN 18533 W1.1-E, W1.2-E, W2.1-E and waterproof concrete to DIN 1045. Includes 2-component resin RESINATOR.

**Scope of delivery**

* 1 piece of 2LINE MIS25
* 1 piece of RESINATOR dual syringe, 25 ml
* 1 piece of wall terminator element

**Material**

Membrane sleeve: TPE

Foil flange: Aluminium-plastic composite foil with butyl rubber

Wall terminator element: PCFR

**Dimensions**

Area of application: 1 fibre-optic cable with Øa 6 - 13 mm

for drill holes Øi: 25 mm

for wall thicknesses starting from 150 mm

**Article Code**

2LINE MIS25 1x6-13 PRO

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99