**Membrane injection system**

for buildings without a basement

For sloping entry through the wall or floor slab in all common types of wall in load case DIN 18533 and waterproof concrete to DIN 1045. Including wall rosette and wall terminator element, 2-component resin Resinator (150 ml).

**Scope of delivery**

* 1 piece of MIS60S
* 1 piece of wall terminator element
* 1 piece of wall rosette

**Material**

Flange, seal insert, counter-bearing and adapter: EPDM

Resin injection hose: PE

Wall rosette: PE

Pipe: PVC-U

Wall terminator element: Flame-retardant polycarbonate

**Dimensions**

For core drills Ø: 62 - 65 mm

Overall length: 1300 mm

**Article Code**

MIS60S E SET

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99