**2LINE Hermes BOX**

Customer line termination

* Holds up to 6 couplings and 24 splices
* Storage capacity of 6x SC pigtails or 6x E2000 pigtails or 12x LC pigtails
* Cable/tube entry max. ø 12mm from below
* Possibility to use commercially available sealing elements in the housing
* Cover closure self-locking and grooved or Torx screw and sealable
* Hinged, latching cover
* UV- and weather resistant
* Fibre routing according to bending radii with the possibility of depositing excess fibre lengths
* Exchangeable splice holder for storing shrink or crimp splice protection elements

**Scope of delivery**

* Wall fixation material
* Optional: Adapters and pigtails included, customer logo, 2LINE ZAF

**Tests/Standards**

Impact resistance class IP54 (for internal adapters)

Impact resistance class IP20 (for external adapters)

Fire resistance class UL94 V-0

**Material**

Plastic, color RAL9003

**Dimensions**

HxWxD[mm]: 235x155x35

**Article Code**

2LINE Hermes BOX

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99