**2LINE Zelos BOX**

Customer line termination

* Holds up to 12 couplings and 24 splices
* Storage capacity of 12x SC pigtails or 12x E2000 pigtails or 24x LC pigtails
* Cable/tube entry max. ø 13mm from below
* Possibility to use commercially available sealing elements in the housing
* Cover closure self-locking and grooved or Torx screw and sealable
* Hinged, latching cover
* Possibility to add on to increase capacity
* Fibre routing according to bending radii with the possibility of depositing excess fibre lengths
* Exchangeable splice holder for storing shrink or crimp splice protection elements

**Scope of delivery**

* Wall fixation material
* Optional: adapter and pigtails included, 2LINE ZAF, customer logo, lock for protection against unauthorized access

**Tests/Standards**

Impact resistance class IP54 (for internal adapters)

Impact resistance class IP20 (for external adapters)

Fire resistance class UL94 V-0

**Material**

Plastic, color RAL9003

**Dimensions**

HxWxD[mm]: 300x194x64

**Article Code**

2LINE Zelos BOX

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99