**2LINE Customer Outlet Box COB**

Optic fibre management system

* Cable entry from below
* Removable lid incl. lock and key
* Loose tube excess length deposit with loop possibility
* Sealed modular base plates: with variable cable entry inserts for diameters from 3 to 20mm alternatively with brush strips
* Use of E&MMS cassettes with the possibility of holding splitters for crimp or shrink splice protection

**Scope of delivery**

* Adapters and pigtails (optional)
* Cable bushings (Ø1.5 - 35mm) (optional)
* Splice cassettes (crimp or shrink splice protection) (optional)
* Cassettes with PLC splitters (optional)
* Patch panel for max. 84 couplings (optional)
* ZEA (central interception element) (optional)
* 1 pc. 2LINE COB L

**Tests/Standards**

Impact resistance class IP54

**Material**

Galvanized steel, plastic, RAL7035

**Dimensions**

HxWxD[mm]: 440x640x150

**Article Code**

2LINE COB L

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99