**2LINE Network Distributor NVt 24**

Fibre optic network distributor

**Scope of delivery**

* 1 pc. 2LINE NVt 24
* Splice cassette system 1-row with max. 36 locking places for up to 432 crimp splice or 432 shrink splice protection trays
* Sealed base plate with draught excluder for outlet area

**Varianten**

: NVt 48

**Tests/Standards**

Environmental protection class IP54

Security level Intrusion resistance: Tested in accordance with RC2 DIN EN 1627

**Material**

Polycarbonate

**Dimensions**

Housing incl. base HxWxD[mm]: 1635x308x215

**Article Code**

2LINE NVt 48

**Article number**

22140

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99