**2LINE Athene KÜB**

Cable overlength box

* Can be used in combination with the 2LINE Athene BOX
* Enables excess length compensation of cascaded cable whips
* Used for depositing excess cable lengths
* Micro tube acceptance of Ø5 /Ø7 /Ø10 mm
* Use of gas/water - stop
* Self-locking closure

**Scope of delivery**

* Cable ties
* Wall fixation material (Universal plugs and screws)
* Optional: customer logo

**Tests/Standards**

Impact resistant IK07

Self-extinguishing according to UL94 V0 and UV-resistant

**Material**

Plastic, signal white RAL 9003

**Dimensions**

HxWxD[mm]: 90x96x27

**Article Code**

2LINE Athene KÜB

**Article number**

21073

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99