**Insertion unit**

For attaching to the basic component

For screwless fixing via latching function. Possibility to insert and remove up to 4 micropipes with diameters of 7, 10 or 12 mm. Openings are sealed at the factory.

**Scope of delivery**

**Material**

ABS

**Article Code**

2LINE G-BOX EFT

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99