**2LINE Helios BOX**

Customer line termination

* Accommodates up to 13 couplings (LC duplex, SC or E2000)
* Holds 28 crimp or 14 shrink splices
* Can be expanded to 112 crimp splices or 98 heat-shrink splices by installing 7 cassettes
* Separation between patch and splice area through inner cover
* Optimised for installations with pre-assembled cables
* Versatile options for loose tube and cable overlength storage

**Scope of delivery**

* 2LINE Helios BOX
* mounting material
* assembly instructions via QR code
* inner lid (optional)
* couplings and pigtails (optional)
* lock (optional)
* splice cassettes (optional)
* label (printing according to customer requirements possible) (optional)

**Tests/Standards**

self-extinguishing according to UL94 V0

protection class IP54

**Material**

plastic PC / ABS, signal white RAL 9003

UV-resistant

**Dimensions**

HxWxD [mm]: 384x235x113

**Article Code**

2LINE Helios BOX

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99