**Corrugated pipe**

for above-ground building entry

For protected installation of the fiber optic pipe up to the above-ground house entry.

**Scope of delivery**

**Dimensions**

OD: 25 mm

**Article Code**

WR25 UV

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99