**Eexcess length box**

for installation on the customer&#039;s property

Features: 1 entry pot with cover including fastening material for attaching the corrugated conduit to the cable overlength box. Set includes all parts required for connection to the 2LINE G-BOX for protected laying of the fiber optic cable to the customer building.

**Scope of delivery**

* 2 pieces 2LINE G-BOX corrugated pipe clip
* 1 piece Cover overlength box
* 4 pieces Clip overlength box
* 1 piece insert pot

**Article Code**

2LINE G-BOX UEB

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99