Wall terminator element

For fibre-optic building entry

Wall terminator element suitable for fibre-optic building entry. For safe rerouting of fibre-optic micropipes inside buildings. Fixation of micropipe without additional cable ties possible.

Scope of delivery

includes required screws and dowels


Material

ABS

Dimensions

Length x width x height: 200 mm x 71 mm x 53 mm

Article Code
GFH WAE

Brand: ZweiCom-Hauff GmbH
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