**2LINE Optical Distribution Frame ODF 180 Active**

Optical distribution frame

* Option for symmetric-inverted construction
* Possible choice for disassembled or preassembled delivery
* Expansion with 19" components
* Depth-adjustable 19" rails
* Integrated patch cable management
* Grounding option
* Height-adjustable frame base
* Fixation on the wall, on the ceiling, back to back or side by side
* Patch cable routing through cable duct on base frame or optionally on roof frame
* Top cabling entry

**Scope of delivery**

* 2LINE Cable duct system top and bottom (optional)
* 2LINE Depth adapter for increasing the installation depth (optional)
* 2LINE ODF door set, 2-piece with 3-point rod locking system, swivelling lever prepared for profile half cylinder (optional)
* 2LINE ODF side panel (optional)
* 1 pc. 2LINE ODF 180 Active
* 1 pc. Assembly instruction

**Material**

Stainless steel, steel galvanized and powder coated in RAL7035, plastic

**Dimensions**

HxWxD[mm]: 1800x900x300

**Article Code**

2LINE ODF 180 Active

Brand: ZweiCom-Hauff GmbH

**Hauff-Technik GRIDCOM GmbH**

**Manufacturer information**

Hauff-Technik GRIDCOM GmbH

Geiselroter Heidle 1

73494 Rosenberg, GERMANY

Telefon +49 79 67 90 08 - 30

Fax +49 79 67 90 08 - 99